A yellow sign with black text

Description automatically generatedCaution: Risk of Shock. Before Opening or Uninstalling the Computer System from Rack, ensure power has been removed from Power Supply(s) as applicable.

ESD Warning: Do not open the Computer System without proper ESD protective equipment and/or anti-static precautions in place.

Warning: As a result of this procedure, BIOS defaults will be loaded; any custom BIOS settings will need to be re-applied while returning the unit to service. Please note any custom settings before proceeding.

1. Chassis Cleaning
   1. For Cleaning procedures, please refer to this Video:  
      [Routine Maintenance for Trenton Systems Products - YouTube](https://www.youtube.com/watch?v=uchxt_W_Oig)
   2. General procedure:
      1. Use canned compressed air to remove dust and debris from the front filter(s) [model dependent] accessible via the front face.
         1. NOTE: Do not use air from an air compressor system that does not have static-arresting equipment.
      2. Host Boards may be removed from backplanes for cleaning. Motherboard based systems should not be removed from the chassis and be cleaned via compressed air in-situ.
      3. Check and Clean the Power Supply fan(s) if applicable.
      4. Check and Clean the rear I/O area to ensure air egress.